|  |  |
| --- | --- |
| **Hazardous Waste Management Checklist** | **Done** |
| All hazardous waste streams generated have been identified and appropriately separated from regular wastes. | □ |
| All applicable environmental permits relating to hazardous waste generation and disposal have been obtained. | □ |
| Hazardous wastes are being collected by a fully licensed waste handler and records (i.e. waste manifests) disposal are fully maintained on-site. | □ |
| Hazardous wastes are being stored in areas that have all required safety features and protections including: * Impervious surfaces and secondary containment.
* Proper signage and labels on all waste containers.
* Protection measures from fire risks.
* Area is well ventilated.
* Wastes are protection from direct sunlight or other weather conditions.
* Only authorized persons are able to access storage areas.
* Spill clean-up equipment is readily available.

  | □ |
| Workers required to handle hazardous wastes are wearing the appropriate PPE. | □ |
| An emergency shower and/or eyewash station is located near the location hazardous wastes are being handled. | □ |