|  |  |
| --- | --- |
| **Hazardous Waste Management Checklist** | **Done** |
| All hazardous waste streams generated have been identified and appropriately separated from regular wastes. | □ |
| All applicable environmental permits relating to hazardous waste generation and disposal have been obtained. | □ |
| Hazardous wastes are being collected by a fully licensed waste handler and records (i.e. waste manifests) disposal are fully maintained on-site. | □ |
| Hazardous wastes are being stored in areas that have all required safety features and protections including:   * Impervious surfaces and secondary containment. * Proper signage and labels on all waste containers. * Protection measures from fire risks. * Area is well ventilated. * Wastes are protection from direct sunlight or other weather conditions. * Only authorized persons are able to access storage areas. * Spill clean-up equipment is readily available. | □ |
| Workers required to handle hazardous wastes are wearing the appropriate PPE. | □ |
| An emergency shower and/or eyewash station is located near the location hazardous wastes are being handled. | □ |